,Standby Power##ELECTRICAL_WATTAGE##WATTS,Sap Code##OTHER##,Rating##OTHER##,Photometric Web File##OTHER##,Mass##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Emergency luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Emergency Charging Power##ELECTRICAL_WATTAGE##WATTS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Earthing Class##OTHER##,Earth Present##OTHER##,Circuit Watts##ELECTRICAL_WATTAGE##WATTS
IQ WAVE LED3100-830 HFIX E3 Q597 MRE,0.15,92900336,30,IQ WAVE LED3100-830 HFIX E3 Q597 MRE.IES,4.4,2950,3000,300,2,98,1,1,30
IQ WAVE LED3100-840 HFIX E3 Q597 MRE,0.15,92900290,30,IQ WAVE LED3100-840 HFIX E3 Q597 MRE.IES,4.4,3100,4000,300,2,103,1,1,30
IQ WAVE LED3100-865 HFIX E3 Q597 MRE,0.15,92900308,30,IQ WAVE LED3100-865 HFIX E3 Q597 MRE.IES,4.4,3100,6500,300,2,103,1,1,30
IQ WAVE LED4100-830 HFIX E3 Q597 MRE,0.15,92900340,40.5,IQ WAVE LED4100-830 HFIX E3 Q597 MRE.IES,4.4,3900,3000,300,2,96,1,1,40.5
IQ WAVE LED4100-840 HFIX E3 Q597 MRE,0.15,92900266,40.5,IQ WAVE LED4100-840 HFIX E3 Q597 MRE.IES,4.4,4100,4000,300,2,101,1,1,40.5
