,Sap Code##OTHER##,Rating##OTHER##,Photometric Web File##OTHER##,Mass##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Circuit Watts##ELECTRICAL_WATTAGE##WATTS
EYE VS LED400-830 HF S ANT,96628455,7,EYE VS LED400-830 HF S ANT.IES,2.5,400,3000,57,7
EYE VS LED400-840 HF S ANT,96665854,7,EYE VS LED400-840 HF S ANT.IES,2.5,435,4000,62,7
EYE VS LED400-830 MWS RF S ANT,96666051,7,EYE VS LED400-830 MWS RF S ANT.IES,2.45,400,3000,57,7
EYE VS LED400-840 MWS S ANT,96665855,7,EYE VS LED400-840 MWS S ANT.IES,2.6,435,4000,62,7
EYE VS LED700-830 HF S ANT,96628456,11,EYE VS LED700-830 HF S ANT.IES,2.5,640,3000,58,11
EYE VS LED700-840 HF S ANT,96665870,11,EYE VS LED700-840 HF S ANT.IES,2.5,700,4000,64,11
EYE VS LED700-830 MWS RF S ANT,96666057,11,EYE VS LED700-830 MWS RF S ANT.IES,3.4,640,3000,58,11
EYE VS LED700-840 MWS S ANT,96665871,11,EYE VS LED700-840 MWS S ANT.IES,2.6,700,4000,64,11
